**Notes**

1. Centres are to complete dimensions details to suit locality
2. All items with red borders are to be pre-fixed prior to assessment
3. Steel conduit must set down to saddle from trunking
4. Trunking bend may be pre-manufactured
5. Tray is to set down to be flushed with wall at this point
6. Pre-fixed tray support brackets to space tray off wall by a minimum of 15 mm
7. Running coupler to allow join to fixed item
8. Conduit to terminate in DB at side or top depending on space restrictions