201: Health and safety in building services engineering  
**Worksheet 5: Safe isolation**

**Answer guide**

In the space below list the steps to take when carrying out a safe isolation procedure.

|  |
| --- |
| * Locate the correct Isolation device. * Check your test equipment. * Prove your test equipment. * Switch off. * Lock and secure Isolation device. * Post warning notices. * Verify that the circuit and equipment are ‘**dead**’. * Prove your test equipment. * Satisfactory? If yes then begin work. |